
	
	                                                               


	
Tender text 
Motion detector theMura S180-100 2W B UP
Order No. white: 		2060770

Features: 
· Passive infra-red motion detector for wall mounting in flush-mounted box
· Cover in Theben design
· Automatic presence and brightness-dependent control for lighting in combination with a staircase light timer switch from Theben (only 4-conductor switching) 
· Rectangular detection area 170°, max. 14 m x 17 m
· Area restriction in scope of delivery
· Mixed light measurement suitable for fluorescent lamps (FL/PL/ESL), halogen/incandescent lamps and LEDs
· Integrated button (can be deactivated)
· Adjustable brightness switching value, teach-in function
· Pulse function for staircase light timer switch, time delay is set at the staircase light timer switch
· Ready for immediate use due to factory presetting 
· Test mode for checking the detection area
· Extension of detection area via parallel switching

Technical data:
Operating voltage: 		230 V AC
Frequency: 			50 – 60 Hz
Power consumption: 		approx. 0.4 W
Radial detection area: 		12 x 10 m
Tangential detection area: 	14 x 17 m
Installation height Mh: 		0.8 – 1.2 m
Brightness switching value: 	5 – 1000 lux
Lighting time delay: 		pulse, time delay is set at the staircase light timer switch
Protection rating: 		IP20
Operating temperature: 		-15 °C to +45 °C
Dimensions: 			85 x 85 mm, installation depth 37 mm
Installation: 			wall mounting in flush-mounted box size 1













Optional accessories:


Cover theMura FED WH
White colour, design to match Feller EDIZIOdue
for details see www.theben.de/theMura
Order No.:			9070786


Cover theMura LM WH
White colour, design to match Legrand Mosaic
for details see www.theben.de/theMura
Order No.:			9070787


Cover theMura BJBSI WH
White colour, design to match BJE balance SI
for details see www.theben.de/theMura
Order No.:			9070788


Cover theMura JAS WH
White colour, design to match Jung AS 500
for details see www.theben.de/theMura
Order No.:			9070789


Cover theMura MMP WH
White colour, design to match Merten M-Plan
for details see www.theben.de/theMura
Order No.:			9070790


Cover theMura GS WH
White colour, design to match Gira Standard 55
for details see www.theben.de/theMura
Order No.:			9070791


Cover theMura BS WH
White colour, design to match Berker S.1
for details see www.theben.de/theMura
Order No.:			9070792


Cover theMura Theben WH
White colour, Theben-Design
for details see www.theben.de/theMura
Order No.:			9070798




ELPA 1
Staircase light timer switch, electronic
Order No.:			0010002


ELPA 3
Staircase light timer switch, electronic
Order No.:			0030002


ELPA 6
Staircase light timer switch, electronic
Order No.:			0060002


ELPA 6 plus
Staircase light timer switch, electronic
Order No.:			0060003


ELPA 8
Staircase light timer switch, electro-mechanical
Order No.:			0080002


ELPA 041
Flush-mounted staircase light timer switch, electronic
Order No.:			0410002


ELPA 047
Flush-mounted staircase light timer switch, electronic
Order No.:			0470002
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