
	
	                                                               


	
Tender text 
Optical presence detector thePixa P360 KNX UP WH
Order No. white: 		2269200

Features:
· General information:
· Optical presence detector for ceiling installation
· KNX Data Secure
· Rectangular detection area with up to 6 flexible detection zones 
(Total area 11.0 x 15.5 m │171 m2; at 4.5 m installation height)
· Restriction of the detection area via app (thePixa Plug)
· Automatic presence and brightness-dependent control for lighting and HVAC
· Each detection zone has its own light measurement
· Adjustment of brightness measurements via thePixa Plug app
· Configurable sensitivity of sensor
· Distinction between motion and presence
· Parallel switching of multiple presence detectors (Master/Slave or Master/Master)
· Test mode for checking function and detection area via app (thePixa Plug)
· Output of occupancy rate and occupancy density via telegram
· Integrated temperature sensor
· Ceiling installation in flush-mounting box (2-point fixing)
· Surface mounting on ceilings possible with surface frame (option)
· thePixa Plug app for settings and evaluations (iOS/Android)
· KNX firmware update possible (ETS app)
· Sensor firmware update possible (thePixa Plug app)
· 6 channels light, Z1 light – Z6 light:
· Switching or constant lighting control with 6 independent control systems and standby function (orientation light)
· Switching mode with dimmable lighting
· Free switch object with configuration type switching
· Fully or semi-automatic device
· Brightness switching value configurable in lux by using parameters
· Brightness switching value configurable in lux by using parameters and telegram
· Light time delay configurable by using parameters
· Aura effect for better orientation and greater safety
· Manual override by telegram
· 6 channels HKL, Z1 HKL – Z6 HKL:
· Configurable switch-on delay and time delay
· Sending of operating mode
· Separate block telegram
· 6 channels room occupancy, Z1 room occupancy – Z6 room occupancy:
· Output of number of persons
· Control of a fan with up to 3 stages
· 3 configurable thresholds (threshold switch)
Technical data:
Operating voltage: 		230 – 240 V AC, 50 Hz
Input power (230 V):		Day mode: typ. 0.9 W
					Night mode: typ. 1.6 W
Bus voltage KNX:		30 V DC
KNX bus power input: 		< 10 mA
Stationary detection area:	5.0 x 7.0 m (IH 3.0 m)
Moving detection area: 	7.5 m x 10.5 m tangential / radial (IH 3.0 m)
Installation height Mh: 		2.5 – 4.5 m
Brightness switching value:	5 – 3000 lux / measurement off
Brightness set point value: 	5 – 3000 lux / light off
Lighting time delay: 		0 s – 60 min
Lighting standby time:		0 s – 60 min / not active / permanently on
Standby dimming value:	1 – 25%
Presence switch-on delay: 	0 s – 120 min / not active
Presence time delay: 		0 s – 120 min
Temperature sensor:		-15 – +60 °C
Protection rating: 		IP20
Operating temperature: 		-5 °C to +45 °C
Dimensions: 			Ø 860 mm, installation depth 37 mm
Installation: 		ceiling installation in flush-mounted box size 1 or ceiling installation socket 73A
Installation: 			Ceiling installation possible with surface frame thePixa WH

Optional accessories:
Surface frame thePixa WH
Order No. white: 		9070816


Ceiling installation box 68A
Drill diameter 68 mm
Order No.: 			9070992
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