Digital rail mounted elapsed-time counter, width 35 mm (BZ148)
	
Digital rail mounted elapsed-time counter, width 35 mm, counter range up to 99,999.99 hours, progress display, terminal screws, operating voltage 12 - 150V DC/24 - 240 V AC, 50/60 Hz

Deliver, assemble, connect up and set up
...

Make: Theben

Type: BZ 148
Order No.: 1480000

Unit: ST

